# Writing all output to: C:\Users\TooT\Dropbox\Electronique\8 FabLab\DrawDio\DrawDio.log
set pad_wire_necking on
bus diagonal
fanout 5
route 50
clean 2
route 50 16
clean 2
filter 5
recorner diagonal
status_file

